{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"images":33},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"merged":[[0,0,0,10],[1,0,1,9],[2,8,2,9],[3,8,3,9],[4,8,4,9],[5,8,5,9],[6,8,6,9],[7,8,7,9],[8,8,8,9],[9,8,9,9],[10,8,10,9],[11,8,11,9],[12,8,12,9],[13,8,13,9],[14,8,14,9],[15,8,15,9],[16,8,16,9],[17,8,17,9],[18,8,18,9],[19,8,19,9],[20,8,20,9],[21,8,21,9],[22,8,22,9],[23,8,23,9],[24,8,24,9],[25,8,25,9],[26,0,28,0],[26,1,28,1],[26,3,28,3],[26,4,28,4],[26,5,28,5],[26,6,28,6],[26,8,28,9],[29,8,29,9],[30,8,30,9],[31,8,31,9],[32,8,32,9],[33,8,33,9],[34,8,34,9],[35,8,35,9],[37,2,37,3],[37,8,37,9],[38,2,38,3],[38,8,38,9],[39,2,39,3],[39,8,39,9],[40,2,40,3],[40,8,40,9],[41,2,41,3],[41,8,41,9],[42,2,42,3],[42,8,42,9],[43,2,43,3],[43,8,43,9],[44,2,44,3],[44,8,44,9],[45,2,45,3],[45,8,45,9],[46,2,46,3],[46,8,46,9],[47,2,47,3],[47,8,47,9],[48,2,48,3],[48,8,48,9],[49,2,49,3],[49,8,49,9],[51,2,51,3],[51,8,51,9],[52,2,52,3],[52,8,52,9],[53,2,53,3],[53,8,53,9],[54,2,54,3],[54,8,54,9],[55,2,55,3],[55,8,55,9]]}
["2025-2027停车场零星工程招标控制工程量清单"]
["第一部分 标牌类"]
["序号","名称","版面尺寸","单位","数量","总高","工艺","全费用     综合单价  （含税）","简图",null,"备注"]
[1,"收费P牌","0.6m X 1m（双面）","块",1,"3.3m（版面下缘离地2.1m）","1、杆直径5cm（壁厚3mm），框架3cm镀锌矩管（壁厚3mm），钻孔直径15cm，埋入深度20cm，用混凝土填充空隙。\n2、版面1.5mm铝板激光切割折弯，铆钉对铆组装，版面喷绘反光膜。",520,null,null,"/"]
[2,"落地提示牌","0.4m X 0.8m（双面）","块",1,"1m（落地式）","1、框架3cm矩管（壁厚2mm)焊接喷漆，稳固脚架长\n60cm加斜撑，0.4厚镀锌板双面裱反光膜。                                    ",240,null,null,"/"]
[3,"立式禁停标牌","0.8m X 1.2m（单面）","块",1,"3.5m（版面下缘离地2.1m）","1、杆直径5cm（壁厚3mm)，版面1.5mm铝板激光切割折弯。钻孔直径15cm，埋入深度20cm，用混凝土填充空隙。\n2、铝条滑槽加固，抱箍组装，版面贴反光膜。",580,null,null,"/"]
[4,"立式标识牌","0.8m X 0.8m","块",1,"3.1m（版面下缘离地1.9m）","1、杆直径5cm（壁厚3mm)，版面1.5mm铝板激光切割。钻孔直径15cm，埋入深度20cm，用混凝土填充空隙。\n2、铝条滑槽加硬，抱箍组装，版面贴反光膜。",340,null,null,"不需立柱时按50%计费"]
[5,"出入口标牌","D=0.8m","块",1,null,"3mmPVC裱晶彩格反光贴",65,null,null,"/"]
[6,"无人值守提示牌","1.0m X 0.6m               ","块",1,"/","5mmPVC裱晶彩格反光贴",75,null,null,"/"]
[7,"U型隔离栏            ","1200*500mm\\89mm","根",1,"/","1、钢管3mm厚、防锈底漆处理，表面喷黄色、黑色亮光金属磁漆。\n2、钻孔安装时，钻孔直径10cm，用混凝土填充空隙。",80,null,null,"钻孔安装时单价按120%计费"]
[8,"停车泊位编号","500*120mm","组",1,"/","热熔树脂",10.3,null,null,"质保期6个月"]
[9,"隔离柱","114*500mm","根",1,"/","114*500mm，2厚",40,null,null,"钻孔安装时按130%计费"]
[10,"公告牌","350*700mm\n总高1米","块",1,"/","采用25镀锌方管和0.4厚镀锌板，版面贴610喷绘反光膜",130,null,null,"/"]
[11,"五防井盖更换","/","个",1,"/","井盖井圈整体更换",727.55,"/",null,"只更换井盖，计60%费用。"]
[12,"普通铸铁井盖更换","内盖700mm*（D400)","个",1,"/","井盖井圈整体更换",499.57,null,null," "]
[13,"高分子井盖更换","/","个",1,"/","井盖井圈整体更换",339.96,"/",null,"只更换井盖，计50%费用。"]
[14,"指示牌","0.4m X 0.6m","块",1,"/","1.2mm铝板激光切割，贴工程级反光膜。",33,null,null,"0.4*0.6的各类指示通用"]
[15,"停车场提示牌","6m X 1m","块",1,"/","1.2mm铝板激光切割，贴工程级反光膜。",825,null,null,"/"]
[16,"停车场提示牌","4m X 1m","块",1,"/","1.2mm铝板激光切割，贴工程级反光膜。",550,null,null,"/"]
[17,"箭头指示牌","0.9m X 0.3m","块",1,"/","牌子1.2mm铝板激光切割，贴工程级反光膜。",47,null,null,"/"]
[18,"反光护角","800mm高","根",1,"/","橡胶+工程级反光膜。",8,null,null,"/"]
[19,"挡轮器","560*150*100mm","个",1,"/","橡胶+工程级反光膜。",37,null,null,"/"]
[20,"减速带","0.5m X 0.35mX0.04m","块",1,"/","橡胶，黄黑相间",38,null,null,"/"]
[21,"广角镜","0.8m×0.8m","个",1,"/","PC材质,表面镀银膜，抗挤压，耐冲击。",98,null,null,"/"]
[22,"指示牌","0.6m X 0.8m","块",1,"/","1.2mm铝板激光切割，贴工程级反光膜。\n胶贴安装或在已有立柱安装",48,null,null,"/"]
[23,"收费牌","0.6m X 0.8m","块",1,"/","不锈钢面板+腐蚀贴1cm结皮板，镜钉安装。",196,null,null,"/"]
[24,"场内收付码","0.6m X 0.8m                           ","块",1,"/","10mm亚克力UV。",148]
[null,null,"0.5m X 0.7m  ",{"$nulls":4},115.36]
[null,null,"0.4m X 0.6m",{"$nulls":4},80.34,null,null,"/"]
[25,"使用标志","0.1m X 0.15m","块",1,"/","双层亚克力子，标志彩印",18,null,null,"/"]
[26,"标牌维修","/","块",1,"/","/",180,"/",null,"基础损坏维修计60%、立柱修复计40%、其它修复计30%。"]
[27,"标牌拆除移位","/","块",1,"/","包含标牌拆除、运输、重新安装（不含基础）",87,"/","/","包含混凝土基础时计140%"]
[28,"U型杆维修","/","根",1,"/","/",44,"/","/","/"]
[29,"版面更换","2平方以内","块",1,"/","包含旧版拆除、清理，新版面制作安装",88,"/","/","超过2平方的，每平方米增加30%费用，以此类推"]
[30,"U型杆安装","/","根",1,"/","不含材料费",60,"/","/","钻孔安装时按120%计费"]
[31,"运输费","/"," 次",1,"/","市内运输",100,"/","/","单次，包含上下车费用。\n 以微型货车计算"]
["第二部分 路面类"]
[32,"热熔道路标线","平方米",null,1,"/","包含热熔道路标线，泊位标线",39.22,"/",null,"/"]
[33,"水除标线","平方米",null,1,"/","包含热熔道路标线，泊位标线",58.13,"/",null,"/"]
[34,"人行道维修（透水砖，不含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、6cm以内的透水混凝土砖拆除安装，3cm砂浆找平层及粘贴层",92.93,"/",null,"不含拆除时计80%，下同"]
[35,"人行道维修（透水砖，含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、6cm以内的透水混凝土砖拆除安装，15cm混凝土C30基层，3cm砂浆找平层及粘贴层",175.58,"/",null,"基层每增加1cm,单价增加5元。"]
[36,"人行道维修（石材，不含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、4cm以内的石材（花岗石）砖拆除安装，3cm砂浆找平层及粘贴层",205.21,"/",null,"超过4cm的石材每1cm增加10元"]
[37,"人行道维修（石材，含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、4cm以内的石材混凝土砖拆除安装，15cm混凝土C30基层，3cm砂浆找平层及粘贴层",289.52,"/",null,"1、超过4cm的石材每1cm增加10元\n2、基层每增加1cm,单价增加5元。"]
[38,"人行道维修（PC砖，不含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、3cm以内的石材砖拆除安装，3cm砂浆找平层及粘贴层",152.91,"/",null,"/"]
[39,"人行道维修（PC砖，含基层）","平方米",null,1,"/","1、包含人行道拆除，建渣清运，成品保护。\n2、3cm以内的石材混凝土砖拆除安装，15cm混凝土C30基层，3cm砂浆找平层及粘贴层",237.22,"/",null,"/"]
[40,"混凝土路面维修（不含垫层）","平方米",null,1,"/","1、包含路面拆除，建渣清运，养护。\n2、20cm以内的C30混凝土拆除，混凝土浇筑，标线恢复。",163.4,"/",null,"/"]
[41,"混凝土路面维修（含垫层）","平方米",null,1,"/","1、包含路面拆除，建渣清运，养护。\n2、20cm以内的C30混凝土拆除，混凝土浇筑，标线恢复。\n3、包含30cm内的水稳或级配碎石垫层施工",259.68,"/",null,"基层每增加1cm,单价增加3元。"]
[42,"AC沥青混凝土路面维修（不含基层）","平方米",null,1,"/","1、包含路面拆除，建渣清运，养护。\n2、6cm以内的沥青混凝土拆除及恢复，标线恢复。",129.03,"/",null,"1、路面厚度每增加1cm,单价增加10元。\n2、使用SMA沥青混凝土按130%计\n"]
[43,"AC沥青混凝土路面维修（含基层）","平方米",null,1,"/","1、包含路面拆除，建渣清运，养护。\n2、6cm以内的沥青混凝土拆除及恢复，标线恢复。\n3、包含30cm内的水稳基层施工",225.32,"/",null,"1、路面厚度每增加1cm,单价增加10元。基层每增加1cm,单价增加3元。\n2、使用SMA沥青混凝土按130%计\n"]
[44,"透水混凝土","平方米",null,1,"/","10cm以内粗骨料透水混凝土",80.13,"/",null,"/"]
["第三部分 其它维修"]
[45,"人工费（难度大的技术工人）","工日",null,1,"/","/",300,"/",null,"焊接、高压作业等技术要求高的作业"]
[46,"人工费（技术工人）","工日",null,1,"/","/",200,"/",null,"/"]
[47,"人工费（普通工人）","工日",null,1,"/","/",120,"/",null,"/"]
[48,"隔离锥桶","个",null,1,"/","贴反光膜",15,"/",null,"材料费"]
[49,"隔离水马","个",null,1,"/","双面贴反光膜\n含注水或加沙",60,"/",null,"材料费"]

{"sheet":"Sheet2","index":1,"n_rows":4,"n_cols":1,"rows_kept":4}
["清单组价"]
["上次招标控制价"]
["上次招标控制价结合询价调整"]
["询价"]